1. Add noise function

* Noise magnitude should not be defined on a per image basis
* i.e. b1500 scan has inherently lower SNR due to long echo time.
* Simulation should have TE as parameter too
* none of compartment simulation scripts include TE, so signals expressed as relative signal to b=0
* But noise magnitude in this relative signal inherently dependent on SNR of b=0 image (normalisation)